**<<Facility Name>>**

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Activity | Enter readings/conditions found: **P** = Pass **F** = Fail (corrective action req’d) | | | | | | | | | Comments/Corrective Actions |
| Date of inspection |  |  |  |  |  |  |  |  |  |  |
| Inspection performed by |  |  |  |  |  |  |  |  |  |  |
| General condition of prime  mover/generator |  |  |  |  |  |  |  |  |  |  |
| Condition of belts & hoses |  |  |  |  |  |  |  |  |  |  |
| Engine oil level (%) |  |  |  |  |  |  |  |  |  |  |
| Lube oil heater |  |  |  |  |  |  |  |  |  |  |
| Coolant level (%) |  |  |  |  |  |  |  |  |  |  |
| Water pump |  |  |  |  |  |  |  |  |  |  |
| Jacket water heater |  |  |  |  |  |  |  |  |  |  |
| Radiator/hoses |  |  |  |  |  |  |  |  |  |  |
| Electrical system |  |  |  |  |  |  |  |  |  |  |
| Battery condition |  |  |  |  |  |  |  |  |  |  |
| Battery electrolyte level |  |  |  |  |  |  |  |  |  |  |
| Battery specific gravity |  |  |  |  |  |  |  |  |  |  |
| Battery charger |  |  |  |  |  |  |  |  |  |  |
| Exhaust system |  |  |  |  |  |  |  |  |  |  |
| Fuel supply level (%) |  |  |  |  |  |  |  |  |  |  |
| Fuel tank vent(s) |  |  |  |  |  |  |  |  |  |  |

**Emergency Generator – Weekly Inspection Checklist**